[Script Info]
; Script generated by Aegisub 3.2.2
; http://www.aegisub.org/
Title: Default Aegisub file
ScriptType: v4.00+
WrapStyle: 0
ScaledBorderAndShadow: yes
YCbCr Matrix: PC.601
PlayResX: 320
PlayResY: 240

[Aegisub Project Garbage]
Audio File: C:/Users/ts/Desktop/图片/MC999 1/P1140399.MOV
Video File: C:/Users/ts/Desktop/图片/MC999 1/P1140399.MOV
Video AR Mode: 4
Video AR Value: 1.333333
Scroll Position: 6
Active Line: 16
Video Position: 1723

[V4+ Styles]
Format: Name, Fontname, Fontsize, PrimaryColour, SecondaryColour, OutlineColour, BackColour, Bold, Italic, Underline, StrikeOut, ScaleX, ScaleY, Spacing, Angle, BorderStyle, Outline, Shadow, Alignment, MarginL, MarginR, MarginV, Encoding
Style: Default,Arial,20,&H00FFFFFF,&H000000FF,&H00000000,&H00000000,0,0,0,0,100,100,0,0,1,2,2,2,10,10,10,1

[Events]
Format: Layer, Start, End, Style, Name, MarginL, MarginR, MarginV, Effect, Text
Dialogue: 0,0:00:00.00,0:00:03.00,Default,,0,0,0,,After power, D1 3 blinks, Enter the "work mode"
Dialogue: 0,0:00:04.00,0:00:07.00,Default,,0,0,0,,D2 on Reversal,D2 Off Forward
Dialogue: 0,0:00:07.00,0:00:20.00,Default,,0,0,0,,Press and hold the Key for 2 seconds,D1 on,enter the "setup mode"
Dialogue: 0,0:00:21.00,0:00:23.00,Default,,0,0,0,,D2 off, It's forward "setup mode"
Dialogue: 0,0:00:24.00,0:00:29.00,Default,,0,0,0,,In forward "setup mode", the continuous trigger KEY twice ,D1 off,entry "Standby timer mode"
Dialogue: 0,0:00:30.00,0:00:33.00,Default,,0,0,0,,In the "Standby timer mode" ,trigger KEY start timing(entry "Timing Mode")
Dialogue: 0,0:00:31.00,0:00:35.00,Default,,0,0,0,,D1 flashing said it is timing("Timing Mode")
Dialogue: 0,0:00:36.00,0:00:39.00,Default,,0,0,0,,Trigger KEY again to stop the clock(exit "Timing Mode")
Dialogue: 0,0:00:36.00,0:00:39.00,Default,,0,0,0,,D1 flashing time is forward time(T1)
Dialogue: 0,0:00:41.00,0:00:44.00,Default,,0,0,0,,Press and hold the Key for 2 seconds,D2 on,enter the Reverse "setup mode"
Dialogue: 0,0:00:44.00,0:00:48.00,Default,,0,0,0,,In Reverse "setup mode", the continuous trigger key twice ,D1 off,entry "Standby timer mode"
Dialogue: 0,0:00:48.00,0:00:50.00,Default,,0,0,0,,In the "Standby timer mode" ,trigger KEY start timing(entry "Timing Mode")
Dialogue: 0,0:00:49.00,0:00:51.00,Default,,0,0,0,,D1 flashing said it is timing("Timing Mode")
Dialogue: 0,0:00:51.00,0:00:55.00,Default,,0,0,0,,Trigger KEY again to stop the clock(exit "Timing Mode")
Dialogue: 0,0:00:52.00,0:00:55.00,Default,,0,0,0,,D1 flashing time is Reverse time(T2) 
Dialogue: 0,0:00:54.00,0:00:58.00,Default,,0,0,0,,So far, forward time(T1) and reverse time(T2) is set up
Dialogue: 0,0:00:54.00,0:00:58.00,Default,,0,0,0,,Re-power in "work mode"
